{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["R001"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"R001","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"cut":false,"hidden":false,"merged":[[12,1,13,1],[12,2,13,2],[12,3,13,3],[11,1,11,8],[2,1,2,8],[3,1,3,8],[9,1,9,8],[5,1,6,1],[5,2,6,2],[5,3,6,3],[7,1,8,1],[7,2,8,2],[5,4,6,4],[5,5,6,7],[5,8,6,8],[7,8,8,8],[7,3,8,3],[7,4,8,4],[7,5,8,7]]}
[]
[]
[null,"→コイルのインダクタンスと周波数からリアクタンスを計算"]
[null,"→リアクタンスを求める関数は lreact(L, f) "]
[]
[null,"L_インダクタンス",0.3,"uH","=",{"$f":"IF(D6=\"mH\",C6*10^-3,IF(D6=\"uH\",C6*10^-6,IF(D6=\"nH\",C6*10^-9,IF(D6=\"pH\",C6*10^-12,C6))))","v":2.9999999999999999E-7},null,null,"H"]
[]
[null,"f_周波数",13.56,"MHz","=",{"$f":"IF(D8=\"KHz\",C8*10^3,IF(D8=\"MHz\",C8*10^6,IF(D8=\"GHz\",C8*10^9,C8)))","v":13560000},null,null,"Hz"]
[]
[]
[]
[null,"→例として上記のリアクタンスを求める場合"]
[null,"→XL=",{"$f":"lreact(F6,F8)","v":25.559997829606555},"j"]
[]
[]
[null,"http://electricrf.net/"]