{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["R001"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"R001","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[[6,1,6,2],[6,3,6,4],[6,5,6,6],[7,5,8,6],[11,5,12,5],[11,1,12,1],[11,2,12,2],[11,4,12,4],[10,1,10,8],[2,1,2,8],[3,1,3,8],[4,1,4,8],[7,1,8,2],[7,3,8,4]]}
[]
[]
[null,"→R+Xjに対するZoΩの場合の正規化反射係数を計算する関数"]
[null,"→正規化反射係数の実部Uを求める関数はrefux(R1, X1, Zo)"]
[null,"→正規化反射係数の虚部Vを求める関数はrefvy(R1, X1, Zo)"]
[]
[null,"R1",null,"X1",null,"Zo"]
[null,0.5,null,10,null,50]
[]
[]
[null,"→例として上記の正規化反射係数U,Vを求める場合"]
[null,"→U=",{"$f":"refux(B8,D8,F8)","v":-0.90548061503631727},null,"→V=",{"$f":"refvy(B8,D8,F8)","v":0.37732289406659753}]
[]
[]
[null,"http://electricrf.net/"]